(module BHC-CR123A (layer F.Cu) (tedit 58A17BC7)
  (descr http://www.challengeelectronics.com/downloads/battery_accessories/lithium/BHC-CR123A.pdf)
  (tags "CR123A Battery")
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value BHC-CR123A (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 10 -5.2) (end 14 -5.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 -4.8) (end 10 -5.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 14 -4.8) (end 10 -4.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 14 -5.2) (end 14 -4.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -12.2 -7) (end -12.2 -5.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -11.8 -7) (end -12.2 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start -11.8 -5.2) (end -11.8 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start -10 -5.2) (end -11.8 -5.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -10 -4.8) (end -10 -5.2) (layer F.SilkS) (width 0.15))
  (fp_line (start -11.8 -4.8) (end -10 -4.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -11.8 -3) (end -11.8 -4.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -12.2 -3) (end -11.8 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -12.2 -4.8) (end -12.2 -3) (layer F.SilkS) (width 0.15))
  (fp_line (start -14 -4.8) (end -12.2 -4.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -14 -5.2) (end -14 -4.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -12.2 -5.2) (end -14 -5.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 17.5 -9) (end 17.5 9) (layer F.SilkS) (width 0.15))
  (fp_line (start 21.5 9) (end -21.5 9) (layer F.SilkS) (width 0.15))
  (fp_line (start 21.5 -9) (end 21.5 9) (layer F.SilkS) (width 0.15))
  (fp_line (start -17.5 -9) (end -17.5 9) (layer F.SilkS) (width 0.15))
  (fp_line (start 21.5 -9) (end -21.5 -9) (layer F.SilkS) (width 0.15))
  (fp_line (start -21.5 -9) (end -21.5 9) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at -19 0) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 19 0) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -12.1 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 12.1 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -19 -8.2) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
)
