Cmp-Mod V01 Created by Cvpcb (2015-02-06 BZR 5410)-product   date = Mon 09 Feb 2015 04:12:04 PM PST

BeginCmp
TimeStamp = /58E6309C;
Reference = AC5;
ValeurCmp = W237-102;
IdModule  = W237-102;
EndCmp

BeginCmp
TimeStamp = /58E631C8;
Reference = ANALOG_IO5;
ValeurCmp = PINHD-2X01_2.54;
IdModule  = 2X01;
EndCmp

BeginCmp
TimeStamp = /58E63290;
Reference = C1;
ValeurCmp = C5/2.5;
IdModule  = C5B2.5;
EndCmp

BeginCmp
TimeStamp = /58E63358;
Reference = C2;
ValeurCmp = C5/2.5;
IdModule  = C5B2.5;
EndCmp

BeginCmp
TimeStamp = /58E63420;
Reference = C3;
ValeurCmp = C5/2.5;
IdModule  = C5B2.5;
EndCmp

BeginCmp
TimeStamp = /58E634E8;
Reference = C4;
ValeurCmp = C5/2.5;
IdModule  = C5B2.5;
EndCmp

BeginCmp
TimeStamp = /58E635B0;
Reference = DALLASTMP5;
ValeurCmp = 78LXX;
IdModule  = 78LXX;
EndCmp

BeginCmp
TimeStamp = /58E63678;
Reference = FUSE5;
ValeurCmp = FUSETE5;
IdModule  = TE5;
EndCmp

BeginCmp
TimeStamp = /58E63740;
Reference = HLK-PM01;
ValeurCmp = HKLPM01;
IdModule  = HKLPM01;
EndCmp

BeginCmp
TimeStamp = /58E63808;
Reference = JP2;
ValeurCmp = PINHD-2X07_2.54;
IdModule  = 2X07;
EndCmp

BeginCmp
TimeStamp = /58E638D0;
Reference = LE33ACZ5;
ValeurCmp = 78LXX;
IdModule  = 78LXX;
EndCmp

BeginCmp
TimeStamp = /58E63998;
Reference = M1;
ValeurCmp = ARDUINO-PRO-MINI-3.3V#NP;
IdModule  = ARDUINO-PRO-MINI#NP;
EndCmp

BeginCmp
TimeStamp = /58E63A60;
Reference = NRF24L01+5;
ValeurCmp = WIRELESS-NRF24L01;
IdModule  = WIRELESS-NRF24L01;
EndCmp

BeginCmp
TimeStamp = /58E63B28;
Reference = RAW_MYSX5;
ValeurCmp = PINHD-1X02_2.54-S;
IdModule  = 1X02-S;
EndCmp

BeginCmp
TimeStamp = /58E63BF0;
Reference = SECUR.5;
ValeurCmp = R-EU_0204/5;
IdModule  = 0204_5;
EndCmp

BeginCmp
TimeStamp = /58E63CB8;
Reference = TERMALFUSE5;
ValeurCmp = FUSETE5;
IdModule  = TE5;
EndCmp

BeginCmp
TimeStamp = /58E63D80;
Reference = VARISTOR5;
ValeurCmp = VARISTOR-7_5;
IdModule  = R-7_5;
EndCmp

EndListe