# KiCad BOM Example 5

# /home/simon/repo/mysensors/water_eink_sensor/schematics/water_eink_sensor.sch

fre 14 dec 2018 18:40:52

Eeschema 5.0.1-33cea8e~68~ubuntu18.04.1

Component Count:12

Ref | Qnty | Value | Part | Footprint | Description | Vendor
--- | --- | --- | --- | --- | --- | ---
BT1 | 1 | Battery_Cell | water_eink_sensor-rescue:Battery_Cell | BH123A:Battery cell CR2 |  |
C1 | 1 | 10nF | water_eink_sensor-rescue:C | Capacitors_SMD:C_0603_HandSoldering |  |
C2 | 1 | 10uF | water_eink_sensor-rescue:C | Capacitors_SMD:C_0603_HandSoldering |  |
J1 | 1 | Eink | Connector_Generic:Conn_01x07 | Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm | Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/) |
J2 | 1 | data | Connector_Generic:Conn_01x05 | Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm_SMD_Pin1Left | Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/) |
J3 | 1 | Program | water_eink_sensor-rescue:CONN_01X04 | Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm_SMD_Pin1Right |  |
L1 | 1 | 10uH | pspice:INDUCTOR | Inductor:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder | Capacitor symbol for simulation only |
L2 | 1 | 15nH | pspice:INDUCTOR | Inductor:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder | Capacitor symbol for simulation only |
R1 | 1 | 4.7k1 | water_eink_sensor-rescue:R | Resistors_SMD:R_0603 |  |
U1 | 1 | E73-2G4M04S-52832 | RF_Module1:E73-2G4M04S-52832 | RFmodule:E73-2G4M04S | nRF52832 BLE5 Module |
U2 | 1 | DS18B20 | Sensor_Temperature1:DS18B20 | Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm | Programmable Resolution 1-Wire Digital Thermometer TO-92 |
U3 | 1 | Ai-Thinker-Ra-01 | RF_Module:Ai-Thinker-Ra-01 | RFmodule:HOPERF_RFM9XW_SMD | Ai-Thinker LoRa Module Ra-01 |