(export (version D)
  (design
    (source /home/simon/repo/mysensors/temp_hum_sensor/schematics_nrf52/temp_hum/temp_hum.sch)
    (date "tor 20 dec 2018 11:47:03")
    (tool "Eeschema 5.0.2-bee76a0~70~ubuntu18.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source temp_hum.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref BT1)
      (value Battery_Cell)
      (footprint mysensors_arduino:CR2450)
      (datasheet ~)
      (libsource (lib Device) (part Battery_Cell) (description "Single-cell battery"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C1904BC))
    (comp (ref J2)
      (value Program)
      (footprint Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm_SMD_Pin1Left)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C190731))
    (comp (ref J1)
      (value Data)
      (footprint Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm_SMD_Pin1Left)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x05) (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C190867))
    (comp (ref C1)
      (value 22uF)
      (footprint Capacitors_SMD:C_0603_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C190AC1))
    (comp (ref U1)
      (value BT832L)
      (footprint Fanstel_modules:BT832-BT832L)
      (libsource (lib Fanstel-modules) (part BT832L) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C19BDF2))
    (comp (ref J3)
      (value Si7021)
      (footprint mysensors_arduino:Si7021)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C1BA02C)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x05)
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x05))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))))
    (libpart (lib Device) (part Battery_Cell)
      (description "Single-cell battery")
      (docs ~)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Fanstel-modules) (part BT832L)
      (footprints
        (fp *BT832L*))
      (fields
        (field (name Reference) U)
        (field (name Value) BT832L)
        (field (name Footprint) BT832_BT832L))
      (pins
        (pin (num P$1) (name P26/SDA) (type BiDi))
        (pin (num P$2) (name P27/SCL) (type BiDi))
        (pin (num P$3) (name P00/XL1) (type BiDi))
        (pin (num P$4) (name P01/XL2) (type BiDi))
        (pin (num P$5) (name P02/AIN0) (type BiDi))
        (pin (num P$6) (name P03/AIN1) (type BiDi))
        (pin (num P$7) (name P09) (type BiDi))
        (pin (num P$8) (name P10) (type BiDi))
        (pin (num P$9) (name VDD) (type BiDi))
        (pin (num P$10) (name GND) (type BiDi))
        (pin (num P$11) (name P13) (type BiDi))
        (pin (num P$12) (name P18) (type BiDi))
        (pin (num P$13) (name P20) (type BiDi))
        (pin (num P$14) (name P21/RESET) (type BiDi))
        (pin (num P$15) (name SWCLK) (type BiDi))
        (pin (num P$16) (name SWDIO) (type BiDi))
        (pin (num P$A0) (name A0/VSS1) (type BiDi))
        (pin (num P$A1) (name A1/P28) (type BiDi))
        (pin (num P$A2) (name A2/P29) (type BiDi))
        (pin (num P$A3) (name A3/P04) (type BiDi))
        (pin (num P$A4) (name A4/P05) (type BiDi))
        (pin (num P$A5) (name A5/P07) (type BiDi))
        (pin (num P$B0) (name B0/VSS2) (type BiDi))
        (pin (num P$B1) (name B1/P25) (type BiDi))
        (pin (num P$B2) (name B2/P30) (type BiDi))
        (pin (num P$B3) (name B3/P31) (type BiDi))
        (pin (num P$B4) (name B4/P06) (type BiDi))
        (pin (num P$B5) (name B5/P08) (type BiDi))
        (pin (num P$C0) (name C0/VSS3) (type BiDi))
        (pin (num P$C1) (name C1/P24) (type BiDi))
        (pin (num P$C2) (name C2/P22) (type BiDi))
        (pin (num P$C3) (name C3/P17) (type BiDi))
        (pin (num P$C4) (name C4/P15) (type BiDi))
        (pin (num P$C5) (name C5/P12) (type BiDi))
        (pin (num P$D0) (name D0/VSS4) (type BiDi))
        (pin (num P$D1) (name D1/P23) (type BiDi))
        (pin (num P$D2) (name D2/P19) (type BiDi))
        (pin (num P$D3) (name D3/P16) (type BiDi))
        (pin (num P$D4) (name D4/P14) (type BiDi))
        (pin (num P$D5) (name D5/P11) (type BiDi)))))
  (libraries
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Fanstel-modules)
      (uri /home/simon/repo/Fanstel-kicad-library/Fanstel-modules.lib)))
  (nets
    (net (code 1) (name "Net-(U1-PadP$B4)")
      (node (ref U1) (pin P$B4)))
    (net (code 2) (name "Net-(U1-PadP$C4)")
      (node (ref U1) (pin P$C4)))
    (net (code 3) (name "Net-(U1-PadP$D4)")
      (node (ref U1) (pin P$D4)))
    (net (code 4) (name "Net-(U1-PadP$A5)")
      (node (ref U1) (pin P$A5)))
    (net (code 5) (name "Net-(U1-PadP$B5)")
      (node (ref U1) (pin P$B5)))
    (net (code 6) (name "Net-(U1-PadP$C5)")
      (node (ref U1) (pin P$C5)))
    (net (code 7) (name "Net-(U1-PadP$D5)")
      (node (ref U1) (pin P$D5)))
    (net (code 8) (name "Net-(U1-PadP$A4)")
      (node (ref U1) (pin P$A4)))
    (net (code 9) (name P02)
      (node (ref U1) (pin P$5))
      (node (ref J1) (pin 5)))
    (net (code 10) (name Tx)
      (node (ref U1) (pin P$7))
      (node (ref J1) (pin 4)))
    (net (code 11) (name "Net-(U1-PadP$3)")
      (node (ref U1) (pin P$3)))
    (net (code 12) (name "Net-(U1-PadP$B2)")
      (node (ref U1) (pin P$B2)))
    (net (code 13) (name "Net-(U1-PadP$C0)")
      (node (ref U1) (pin P$C0)))
    (net (code 14) (name "Net-(U1-PadP$D0)")
      (node (ref U1) (pin P$D0)))
    (net (code 15) (name "Net-(U1-PadP$11)")
      (node (ref U1) (pin P$11)))
    (net (code 16) (name "Net-(U1-PadP$A1)")
      (node (ref U1) (pin P$A1)))
    (net (code 17) (name "Net-(U1-PadP$B1)")
      (node (ref U1) (pin P$B1)))
    (net (code 18) (name "Net-(U1-PadP$C1)")
      (node (ref U1) (pin P$C1)))
    (net (code 19) (name "Net-(U1-PadP$D1)")
      (node (ref U1) (pin P$D1)))
    (net (code 20) (name "Net-(U1-PadP$12)")
      (node (ref U1) (pin P$12)))
    (net (code 21) (name "Net-(U1-PadP$A2)")
      (node (ref U1) (pin P$A2)))
    (net (code 22) (name "Net-(U1-PadP$4)")
      (node (ref U1) (pin P$4)))
    (net (code 23) (name "Net-(U1-PadP$C2)")
      (node (ref U1) (pin P$C2)))
    (net (code 24) (name "Net-(U1-PadP$D2)")
      (node (ref U1) (pin P$D2)))
    (net (code 25) (name "Net-(U1-PadP$13)")
      (node (ref U1) (pin P$13)))
    (net (code 26) (name "Net-(U1-PadP$A3)")
      (node (ref U1) (pin P$A3)))
    (net (code 27) (name "Net-(U1-PadP$B3)")
      (node (ref U1) (pin P$B3)))
    (net (code 28) (name "Net-(U1-PadP$C3)")
      (node (ref U1) (pin P$C3)))
    (net (code 29) (name "Net-(U1-PadP$D3)")
      (node (ref U1) (pin P$D3)))
    (net (code 30) (name "Net-(U1-PadP$14)")
      (node (ref U1) (pin P$14)))
    (net (code 31) (name GND)
      (node (ref BT1) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin P$10))
      (node (ref J3) (pin 2)))
    (net (code 32) (name "Net-(U1-PadP$6)")
      (node (ref U1) (pin P$6)))
    (net (code 33) (name +3V3)
      (node (ref U1) (pin P$9))
      (node (ref C1) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref J3) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref BT1) (pin 1)))
    (net (code 34) (name SCL)
      (node (ref U1) (pin P$2))
      (node (ref J3) (pin 3)))
    (net (code 35) (name SDA)
      (node (ref U1) (pin P$1))
      (node (ref J3) (pin 4)))
    (net (code 36) (name "Net-(U1-PadP$B0)")
      (node (ref U1) (pin P$B0)))
    (net (code 37) (name "Net-(U1-PadP$A0)")
      (node (ref U1) (pin P$A0)))
    (net (code 38) (name SWDCLK)
      (node (ref U1) (pin P$15))
      (node (ref J2) (pin 3)))
    (net (code 39) (name SWDIO)
      (node (ref U1) (pin P$16))
      (node (ref J2) (pin 4)))
    (net (code 40) (name Rx)
      (node (ref J1) (pin 3))
      (node (ref U1) (pin P$8)))))